Backend: 
-add this as next QC step after existing ones, before returning to front end:
1. Ensure all sites features are within the correct cabinet boundary. Make sure the 2-digit number in the cabinet_boundaries feature "Name" field matches the 2-digit number in the "Group 1" field for all sites.
2. Ensure all access_points features are within the correct cabinet boundary. Make sure the 2-digit number in the cabinet_boundaries feature "Name" field matches the 2-digit number in the "Group 1" field for all access_points.
3. Ensure all permits features are within the correct cabinet boundary. Make sure the 2-digit number in the cabinet_boundaries feature "Name" field matches the 2-digit number in the "Group 1" field for all permits features.
4. Ensure all splicing features are within the correct cabinet boundary. Make sure the 2-digit number in the cabinet_boundaries feature "Name" field matches the 2-digit number in the "Group 1" field for all splicing features.
5. Ensure all network_elements features are within the correct cabinet boundary. Make sure the 2-digit number in the cabinet_boundaries feature "Name" field matches the 2-digit number in the "Group 1" field for all network_elements features.
6. Ensure all poles features are within the correct cabinet boundary. Make sure the 2-digit number in the cabinet_boundaries feature "Name" field matches the 2-digit number in the "Group 1" field for all poles features.
7. Ensure all segments features are within the correct cabinet boundary. Make sure the 2-digit number in the cabinet_boundaries feature "Name" field matches the 2-digit number in the "Group 1" field for all access_points. EXCEPTION: If a segment crosses between cabinet_boundaries polygons, don't evaluate it.
8. Ensure NO features are outside of the entirety of the cabinet_boundaries polgyons layer

Like with previous QC efforts, return list of specific issues in the .txt file if it does not pass QC